maximal pulse height difference (normalized)

0 2 4 6 8 10 12 noise [ADC count]

0

2

4

6

8

10 Noise (peak inversion on) versus maximal pulse height difference (peak inversion off)

FNAL UCSB